	RIPRAP BASIN CHECKLIST

	Route
     
Project No.      
Designer
     
Date
     
Reviewer
     
Date
     

	DESIGN VALUES

(IDM Figure 34-8B)
	TRIAL 1
	FINAL TRIAL
	
	BASIN DIMENSIONS
	FEET

	Equivalent Depth, dE
	     
	     
	
	Pool length is the

larger of:
	10hS
	     
	

	D50/dE
	     
	     
	
	
	3Wo
	     
	

	D50
	     
	     
	
	Basin length is the

larger of:
	15hS
	     
	

	Froude No., Fr
	     
	     
	
	
	4Wo
	     
	

	hS/dE
	     
	     
	
	Approach Thickness
	3D50
	     

	hS
	     
	     
	
	Basin Thickness
	2D50
	     

	hS/D50
	     
	     
	
	
	
	
	

	2 < hS/D50 < 4
	     
	     
	
	
	
	
	


	TAILWATER CHECK
	
	DOWNSTREAM RIPRAP (IDM Figure 34-8D)

	Tailwater, TW
	     
	
	L/DE
	L
	VL/Vo
	VL
	D50

	Equivalent depth, dE
	     
	
	     
	     
	     
	     
	     

	TW/dE
	     
	
	     
	     
	     
	     
	     

	IF TW/dE > 0.75, calculate riprap

downstream using IDM Figure 34-8D
	
	     
	     
	     
	     
	     

	
	
	     
	     
	     
	     
	     

	DE = (4Ac/π)0.5
	     
	
	     
	     
	     
	     
	     








