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GRANULAR FILTER
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FABRIC FILTER


PHYSICAL PROPERTIES CLASS:      

HYDRAULIC PROPERTIES:


PIPING RESISTANCE < 50% PASSING 75μm; AOS < 600 μm


PIPING RESISTANCE < 50% PASSING 75μm; AOS < 300 μm

PERMEABILITY:  SOIL PERMEABILITY < FABRIC PERMEABILITY

SELECTED FILTER FABRIC SPECIFICATIONS:      
FILTER DESIGN
_1163503503.unknown
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_1163503497.unknown

