105-C-247 BRIDGE INSPECTION COORDINATION

*(Adopted 01-21-16)*

 The following routine, fracture critical, underwater, or special bridge inspections are due to be performed by the Department’s Bridge Inspection Office, or its authorized representative, on each bridge within the construction limits of the contract.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **StructureNumber** | **NBINumber** | **Location** | **InspectionType** | **LastInspectionDate(MM/DD/YY)** | **Frequency****(Mos.)** | **FirstScheduledInspection(MM/YY)** | **SecondScheduledInspection(MM/YY)** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

 Each bridge inspection shall be identified in the schedule of work in accordance with 108.04. Portions of each bridge replaced, reconstructed, or repaired and subsequently used for maintenance of traffic will be inspected within 90 days of being opened to traffic.

 Notice will be given no less than seven days prior to each bridge inspection. Access, coordination, and cooperation for the required bridge inspections shall be in accordance with 105.05.