805-T-202 ACCESSIBLE PEDESTRIAN SIGNALS WITH SPEECH WALK MESSAGES

*(Adopted 11-22-13)*

Accessible pedestrian push-buttons shall be provided at:

*Name of intersection*

The walk messages used shall be as follows:

|  |  |  |
| --- | --- | --- |
| **Intersection** | **Push-button\*** | **Walk Message\*\*** |
| North leg |  |  |
| South leg |  |  |
| East leg |  |  |
| West leg |  |  |
| **\*** Enter “N/A”, or “APS”  **\*\*** Leave blank, enter “percussive tone” if applicable, or text for speech walk message | | |

**(Leave remainder of this form blank if not applicable)**

      (      leg of intersection)

Walk Message:

      (      leg of intersection)

Walk Message:

Special Instructions: