HOT DRINK MACHINE

Make & Model Number: \_USI GENEVA FREEZE DRIED COFFEE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured hot drink machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Vends freeze-dried regular coffee without modification | X |  |  |
| B. | Vends soluble decaf coffee or soluble hot tea | X |  |  |
| C. | Vends soluble decaf coffee or soluble hot tea | X |  |  |
| D. | Artificial sweetener option available instead of other option |  |  | X |
| E. | Minimum 1 (one) custom select option, such as café mocha | X |  |  |
| F. | Vends a minimum of two (2) soluble gourmet coffee (SGC) | X |  |  |
| G. | Vends a minimum of one (1) hot chocolate selection whipped | X |  |  |
| H. | Minimum 7 different hot beverage selections | X |  |  |
| I. | Two separate cup dispensers vend two different cup sizes |  |  | X |
| J. | Cup sensor or approved equal allows for any style cup | X |  |  |
| K. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| L. | Braille programming capability | X |  |  |
| M. | Text to Voice synthesizer capability to include any necessary wiring harness and software (Handheld, portable voice unit purchased under separate order) |  |  | X |
| N. | Hydro-life water filter, or equivalent, installed in unit | X |  |  |
| O. | Multi-price capability | X |  |  |
| P. | Coin mechanism, installed in unit, 24 -volt MDB | X |  |  |
| Q. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| R. | Minimum 2.5-gallon hot water tank | X |  |  |
| S. | Maximum Overall Dimensions: 72”h x 39” w x 34” d | X |  |  |
| T. | Maximum 120 VAC | X |  |  |
| U. | UL approved | X |  |  |
| V. | Internal outlet, minimum 110v-20amp | X |  |  |
| W. | Minimum 18-gauge steel cabinet | X |  |  |
| X. | Minimum 16-gauge steel door | X |  |  |
| Y. | Self-test system diagnostics | X |  |  |
| Z. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) | X |  |  |
| AA. | Front door security bar installed (optional) |  |  | X |
| BB. | Front door security bar installed (optional) |  |  | X |
| CC. | "T" handle type lock receptacles | X |  |  |
| DD. | Machines must have winterized tape provided for exterior water lines |  |  | X |
| EE. | Full financial & product audit function | X |  |  |
| FF. | ADA Compliant | X |  |  |

5-WIDE SNACK MACHINE (REFRIGERATED)

Make & Model Number: \_\_AMS 39 BOT/FOOD\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 5-wide snack machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge steel cabinet with glass front | X |  |  |
| B. | Minimum 30 selections with 6 shelves | X |  |  |
| - | Snack shelves: 5 selections per tray, minimum 10 products per selection, dual spirals | X |  |  |
| - | Candy shelves: 10 selections per tray, minimum 15 products per selection | X |  |  |
| C. | Optional shelf set-up to meet vendor needs | X |  |  |
| D. | Adjustable rail positions on top 5 shelves for taller products | X |  |  |
| E. | Total cash accountability | X |  |  |
| F. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| G. | Braille programming capability | X |  |  |
| H. | Text to Voice synthesizer capability to include any necessary wiring harness and software.  (Handheld, portable voice unit purchased under separate order) |  |  | X |
| I. | Multi-price capability | X |  |  |
| J. | Adjustable position drive delivery motor | X |  |  |
| K. | Guaranteed delivery sensor | X |  |  |
| L. | Multi-Drop Bus capabilities | X |  |  |
| M. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| N. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| O. | Self-test system diagnostics | X |  |  |
| P. | "T" handle type lock receptacles | X |  |  |
| Q. | Maximum Overall Dimensions: 72”h x 33 1/2” w x 35” d | X |  |  |
| R. | Maximum 120 AC | X |  |  |
| S. | UL approved | X |  |  |
| T. | Optional exhaust fan |  |  | X |
| U. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) | X |  |  |
| V. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| W. | Full financial & product audit function | X |  |  |
| X. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

4-WIDE SNACK MACHINE (REFRIGERATED)

Make & Model Number: \_AMS 35 BOT/FOOD\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 4-wide snack machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge steel cabinet with glass front | X |  |  |
| B. | Minimum 24 selections with 6 shelves | X |  |  |
| - | Snack shelves: 4 selections per tray, minimum 10 products per selection, dual spirals | X |  |  |
| - | Candy shelves: 8 selections per tray, minimum 15 products per selection | X |  |  |
| C. | Optional shelf set-up to meet vendor needs | X |  |  |
| D. | Adjustable rail positions on top 5 shelves for taller products | X |  |  |
| E. | Multi-price capability | X |  |  |
| F. | Total cash accountability | X |  |  |
| G. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| H. | Braille programming capability | X |  |  |
| I. | Text to Voice synthesizer capability to include any necessary wiring harness and software.  (Handheld, portable voice unit purchased under separate order) |  |  | X |
| J. | Adjustable position drive delivery motor | X |  |  |
| K. | Guaranteed delivery sensor | X |  |  |
| L. | Multi-Drop Bus capabilities | X |  |  |
| M. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| N. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| O. | Self-test system diagnostics | X |  |  |
| P. | "T" handle type lock receptacles | X |  |  |
| Q. | Maximum Overall Dimensions: 72”h x 33 1/2” w x 35” d | X |  |  |
| R. | Maximum 120 AC | X |  |  |
| S. | UL approved | X |  |  |
| T. | Optional exhaust fan |  |  | X |
| U. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) | X |  |  |
| V. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| W. | Full financial & product audit function | X |  |  |
| X. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

4-WIDE SNACK MACHINE (OUTSIDE)

Make & Model Number: \_\_\_\_\_NO OPTION\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 5-wide snack machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge steel cabinet with glass front |  |  |  |
| B. | Minimum 30 selections with 6 shelves, 4 snack/2 candy |  |  |  |
| - | Snack shelves: 5 selections per tray, minimum 10 products per selection, dual spirals |  |  |  |
| - | Candy shelves: 10 selections per tray, minimum 15 products per selection |  |  |  |
| C. | Optional shelf set-up to meet vendor needs |  |  |  |
| D. | Adjustable rail positions on top 5 shelves for taller products |  |  |  |
| E. | Multi-price capability |  |  |  |
| F. | Total cash accountability |  |  |  |
| G. | Alpha/numeric type selection keypad w/Braille |  |  |  |
| H. | Braille programming capability |  |  |  |
| I. | Text to Voice synthesizer capability to include any necessary wiring harness and software.  (Handheld, portable voice unit purchased under separate order) |  |  |  |
| J. | Adjustable position drive delivery motor |  |  |  |
| K. | Guaranteed delivery sensor |  |  |  |
| L. | Multi-Drop Bus capabilities |  |  |  |
| M. | Coin mechanism installed in unit, 24-volt MDB |  |  |  |
| N. | Bill acceptor installed in unit, 24-volt MDB |  |  |  |
| O. | Self-test system diagnostics |  |  |  |
| P. | "T" handle type lock receptacles |  |  |  |
| Q. | Maximum Overall Dimensions: 72”h x 33 1/2” w x 35” d |  |  |  |
| R. | Maximum 120 AC |  |  |  |
| S. | UL approved |  |  |  |
| T. | Optional exhaust fan |  |  |  |
| U. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) |  |  |  |
| V. | Internal temperature 35 degrees to 65 degrees |  |  |  |
| W. | Full financial & product audit function |  |  |  |
| X. | ADA compliant |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

5-WIDE SNACK MACHINE (OUTSIDE)

Make & Model Number: \_\_\_AMS 39 VRM\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 5-wide outside snack machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge steel cabinet with glass front | X |  |  |
| B. | Minimum 30 selections with 6 shelves, 4 snack/2 candy | X |  |  |
| - | Snack shelves: 5 selections per tray, minimum 10 products per selection, dual spirals | X |  |  |
| - | Candy shelves: 10 selections per tray, minimum 15 products per selection | X |  |  |
| C. | Optional shelf set-up to meet vendor needs | X |  |  |
| D. | Adjustable rail positions on top 5 shelves for taller products | X |  |  |
| E. | Multi-price capability | X |  |  |
| F. | Total cash accountability | X |  |  |
| G. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| H. | Braille programming capability | X |  |  |
| I. | Text to Voice synthesizer capability to include any necessary wiring harness and software.  (Handheld, portable voice unit purchased under separate order) |  |  | X |
| J. | Adjustable position drive delivery motor | X |  |  |
| K. | Guaranteed delivery sensor | X |  |  |
| L. | Self-test system diagnostics | X |  |  |
| M. | Multi-Drop Bus capabilities | X |  |  |
| N. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| O. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| P. | Maximum Overall Dimensions: 72”h x 33 1/2” w x 35” d | X |  |  |
| Q. | "T" handle type lock receptacles | X |  |  |
| R. | Maximum 120 AC | X |  |  |
| S. | UL approved | X |  |  |
| T. | Optional exhaust fan |  |  | X |
| U. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) | X |  |  |
| V. | Vandal resistant | X |  |  |
| W. | Triple-pane heated glass protected by a layer of durable polyurethane | X |  |  |
| X. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| Y. | Full financial & product audit function | X |  |  |
| Z. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

COLD DRINK MACHINE, GLASS FRONT

Make & Model Number: \_\_5800 BEV MAX CLASSIC\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured cold drink machine/glass front with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 5 delivery trays with a minimum of 9 columns/tray, glass front | X |  |  |
| B. | Minimum 45 selections | X |  |  |
| C. | Capacity: 360-405 products | X |  |  |
| D. | Vends 10oz, 12oz, 16oz, and 20oz PET/glass bottles or cans | X |  |  |
| E. | Hermetic compressor systems construction or approved equivalent | X |  |  |
| F. | Non-CFC, R134A refrigerant or approved equivalent | X |  |  |
| G. | Refrigeration unit serviceable from the front of the machine | X |  |  |
| H. | Display-prompted programming and set-up | X |  |  |
| I. | Multi-pricing capability | X |  |  |
| J. | Self-test system diagnostics | X |  |  |
| K. | Total cash accountability | X |  |  |
| L. | Multi-Drop Bus capabilities | X |  |  |
| M. | Full financial & product audit function | X |  |  |
| N. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| O. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| P. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| Q. | Maximum overall dimensions: 72"h x 47" w x 32"d | X |  |  |
| R. | Maximum 120 VAC | X |  |  |
| S. | UL approved | X |  |  |
| T. | Minimum 16-guage steel cabinet | X |  |  |
| U. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) |  |  | X |
| V. | Text to Voice synthesizer capability to include any necessary wiring harness and software. (Handheld, portable voice unit purchased under separate order) | X |  |  |
| W. | ADA Compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

COLD DRINK MACHINE, GLASS FRONT

Make & Model Number: \_\_\_\_\_\_3800 BEV MAX CLASSIC NARROW\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured cold drink machine/glass front with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 5 delivery trays with a minimum of 7 columns/tray, glass front | X |  |  |
| B. | Minimum 35 selections | X |  |  |
| C. | Capacity: 280-315 products | X |  |  |
| D. | Vends 10oz, 12oz, 16oz, and 20oz PET/glass bottles or cans | X |  |  |
| E. | Hermetic compressor systems construction or approved equivalent | X |  |  |
| F. | Non-CFC, R134A refrigerant or approved equivalent | X |  |  |
| G. | Refrigeration unit serviceable from the front of the machine | X |  |  |
| H. | Display-prompted programming and set-up | X |  |  |
| I. | Multi-pricing capability | X |  |  |
| J. | Self-test system diagnostics | X |  |  |
| K. | Total cash accountability | X |  |  |
| L. | Multi-Drop Bus capabilities | X |  |  |
| M. | Full financial & product audit function | X |  |  |
| N. | Text to Voice synthesizer capability to include any necessary wiring harness and software. |  |  | X |
|  | (Handheld, portable voice unit purchased under separate order) |  |  | X |
| O. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| P. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| Q. | Maximum overall dimensions: 72"h x 47" w x 32"d | X |  |  |
| R. | Maximum 120 VAC | X |  |  |
| S. | UL approved | X |  |  |
| T. | Minimum 16-guage steel cabinet | X |  |  |
| U. | Operations manual shall be available in electronic file format, (Microsoft Word, Excel or digital) | X |  |  |
| V. | ADA Compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

4-WIDE COMBO MACHINE

Make & Model Number: \_\_\_\_\_\_AMS 35 BOT/FOOD\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 4-wide combo snack/drink/food machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge heavy-duty steel cabinet with glass front | X |  |  |
| B. | Capability to dispense can/bottle drinks and food | X |  |  |
| C. | Minimum 20 selections with 5 shelves with dual spirals | X |  |  |
| D. | Optional shelf set-up to meet vendor needs | X |  |  |
| E. | Adjustable rail positions on a minimum of 3 top shelves for taller products | X |  |  |
| F. | Self-test system diagnostics | X |  |  |
| G. | Full financial & product audit function | X |  |  |
| H. | Total cash accountability | X |  |  |
| I. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| J. | Braille programming capability | X |  |  |
| K. | Text to Voice synthesizer capability to include any necessary wiring harness and software. (Handheld, portable voice unit purchased under separate order) |  |  | X |
| L. | Adjustable position drive delivery motor | X |  |  |
| M. | Guaranteed delivery sensor | X |  |  |
| N. | Multi-Drop Bus capabilities | X |  |  |
| O. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| P. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| Q. | Maximum Overall Dimensions: 72”h x 41” w x 36” d | X |  |  |
| R. | Maximum 120 VAC | X |  |  |
| S. | UL approved | X |  |  |
| T. | Optional exhaust fan |  |  | x |
| U. | Operations manual shall be available in electronic file format | X |  |  |
|  | (Microsoft Word, Excel or digital) | X |  |  |
| V. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| W. | "T" handle type lock receptacles | X |  |  |
| X. | ADA compliant | X |  |  |
| Y. | Multi-price capability | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

5-WIDE COMBO MACHINE

Make & Model Number: \_\_\_\_\_AMS 39 BOT/FOOD\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 5-wide combo snack/drink/food machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge heavy-duty steel cabinet with glass front | X |  |  |
| B. | Capability to dispense can/bottle drinks and food | X |  |  |
| C. | Minimum 25 selections with 5 shelves containing dual spirals | X |  |  |
| D. | Optional shelf set-up to meet vendor needs | X |  |  |
| E. | Adjustable rail positions on a minimum of 3 top shelves for taller products | X |  |  |
| F. | "T" handle type lock receptacles | X |  |  |
| G. | Self-test system diagnostics | X |  |  |
| H. | Full financial & product audit function | X |  |  |
| I. | Total cash accountability | X |  |  |
| J. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| K. | Multi-price capability | X |  |  |
| L. | Braille programming capability | X |  |  |
| M. | Text to Voice synthesizer capability to include any necessary wiring harness and software. (Handheld, portable voice unit purchased under separate order) |  |  | X |
| N. | Adjustable position drive delivery motor | X |  |  |
| O. | Guaranteed delivery sensor | X |  |  |
| P. | Multi-Drop Bus capabilities | X |  |  |
| Q. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| R. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| S. | Maximum Overall Dimensions: 72”h x 41” w x 36” d | X |  |  |
| T. | Maximum 120 VAC | X |  |  |
| U. | UL approved | X |  |  |
| V. | Optional exhaust fan |  |  | X |
| W. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) | X |  |  |
| X. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| Y. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

10-SELECT COLD CAN/BOTTLE DRINK MACHINE

Make & Model Number: VENDO 721 BLACK ICE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 10-select cold can/bottle drink machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 10 selections, 10 columns | X |  |  |
| B. | Large package delivery port | X |  |  |
| C. | Double-depth bottle vending | X |  |  |
| D. | Quadruple-depth can vending | X |  |  |
| E. | Minimum 72, 12oz. Cans/column | X |  |  |
| F. | Minimum 34 16oz/20oz PET or glass bottles/column | X |  |  |
| G. | Multi-pricing capability | X |  |  |
| H. | "T" handle type lock receptacles | X |  |  |
| I. | Self-test system diagnostics | X |  |  |
| J. | Total cash accountability | X |  |  |
| K. | Full financial & product audit function | X |  |  |
| L. | CFC free and lint tolerant | X |  |  |
| M. | Multi-drop bus capabilities | X |  |  |
| N. | Optional merchandising door design | X |  |  |
| O. | Stock with door open to 180 degrees | X |  |  |
| P. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| Q. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| R. | Maximum 120 VAC | X |  |  |
| S. | UL/CUL outdoor approval | X |  |  |
| T. | Maximum overall dimensions 72"h x 28"w x 34"d | X |  |  |
| U. | Ability to install locking casters | X |  |  |
| V. | Minimum 16-gauge steel cabinet | X |  |  |
| W. | Text to Voice synthesizer capability to include any necessary wiring harness and software. (Handheld, portable voice unit purchased under separate order) |  |  | X |
| X. | Operations manual shall be available in electronic file format  (Microsoft Word, Excel or digital) | X |  |  |
| Y. | Live display | X |  |  |
| Z. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

8-SELECT COLD CAN/BOTTLE DRINK MACHINE

Make & Model Number: \_\_\_\_\_VENDO 621 WATERFALL\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 8-select cold can/bottle drink machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 8 selections, 8 columns | X |  |  |
| B. | Large package delivery port | X |  |  |
| C. | Double-depth bottle vending | X |  |  |
| D. | Quadruple-depth can vending | X |  |  |
| E. | Multi-pricing capability | X |  |  |
| F. | Minimum 72, 12oz. Cans/column | X |  |  |
| G. | Minimum 34 16oz/20oz PET or glass bottles/column | X |  |  |
| H. | Live display | X |  |  |
| I. | Self-test system diagnostics | X |  |  |
| J. | Full financial & product audit function | X |  |  |
| K. | Total cash accountability | X |  |  |
| L. | CFC free and lint tolerant | X |  |  |
| M. | Multi-drop bus capabilities | X |  |  |
| N. | Optional merchandising door design | X |  |  |
| O. | Stock with door open to 180 degrees | X |  |  |
| P. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| Q. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| R. | Maximum 120 VAC | X |  |  |
| S. | UL/CUL outdoor approval | X |  |  |
| T. | Maximum overall dimensions 72"h x 28"w x 34"d |  |  | X |
| U. | Ability to install locking casters | X |  |  |
| V. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| W. | Minimum 16-gauge steel cabinet | X |  |  |
| X. | Text to Voice synthesizer capability to include any necessary wiring harness and software. (Handheld, portable voice unit purchased under separate order) |  |  | X |
| Y. | Operations manual shall be available in electronic file format (Microsoft Word, Excel or digital) | X |  |  |
| Z. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

COLD/FROZEN COMBO MACHINE

Make & Model Number: \_\_\_\_\_USI ALPINE 3000 COMBI\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured cold/frozen combo machine with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 18-gauge heavy-duty steel cabinet with glass front | X |  |  |
| B. | Minimum 30 selections with 6 shelves | X |  |  |
| C. | Optional shelf set-up to meet vendor needs | X |  |  |
| D. | Adjustable rail positions on top 5 shelves for taller products | X |  |  |
| E. | "T" handle type lock receptacles | X |  |  |
| F. | Self-test system diagnostics | X |  |  |
| G. | Full financial & product audit function | X |  |  |
| H. | Total cash accountability | X |  |  |
| I. | Multi-price capability | X |  |  |
| J. | Alpha/numeric type selection keypad w/Braille | X |  |  |
| K. | Braille programming capability | X |  |  |
| L. | Text to Voice synthesizer capability to include any necessary wiring harness and software. |  |  | X |
| M. | Internal temperature 35 degrees to 65 degrees | X |  |  |
| N. | Adjustable position drive delivery motor | X |  |  |
| O. | Guaranteed delivery sensor | X |  |  |
| P. | Multi-Drop Bus capabilities | X |  |  |
| Q. | Coin mechanism installed in unit, 24-volt MDB | X |  |  |
| R. | Bill acceptor installed in unit, 24-volt MDB | X |  |  |
| S. | Maximum Overall Dimensions: 72”h x 41” w x 36” d | X |  |  |
| T. | Maximum 120 VAC | X |  |  |
| U. | UL approved | X |  |  |
| V. | Optional exhaust fan |  |  | X |
| W. | Operations manual shall be available in electronic file format (Microsoft Word, Excel or digital) | X |  |  |
| X. | ADA compliant | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

MICROWAVE OVEN

Make & Model Number: \_\_\_\_\_\_\_NE-1054F\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured microwave oven with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Minimum 1,000 watts | X |  |  |
| B. | Minimum capacity 0.8 cu.ft. | X |  |  |
| C. | Maximum exterior dimensions: 16'h x 23"w x 20"d | X |  |  |
| D. | Minimum 6-time selections | X |  |  |
| E. | Side-swing door with see-through window | X |  |  |
| F. | No standby operation required | X |  |  |
| G. | Stainless steel interior cavity with quality overall construction | X |  |  |
| H. | Meets all safety performance and sanitation standards for microwave ovens | X |  |  |
|  | of the US Government Department of Health & Human Services, 21 CFR |  |  |  |
|  | sub-chapter J under the authority of the radiation control for the Health |  |  |  |
|  | and Safety Act of 1968 |  |  |  |
| I. | Maximum 120 VAC | X |  |  |
| J. | UL approved | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

BILL CHANGER (3 HOPPER)

Make & Model Number: \_\_\_\_\_\_\_\_MC830-DA CHANGER\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 3-hopper bill changer with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Front loading machine | X |  |  |
| B. | Maximum security design | X |  |  |
| C. | Minimum 14-gauge steel construction | X |  |  |
| D. | "T" handle type lock receptacles | X |  |  |
| E. | Minimum 3 hoppers accommodating: $1 coins, quarters, dimes, and nickels | X |  |  |
| F. | Accepts $1, $5, $10, and $20 bills | X |  |  |
| G. | Accepts Susan B. Anthony and $1 gold coins |  |  | X |
| H. | Hand-held data terminal for programming with braille |  |  | X |
| I. | Battery back-up |  |  | X |
| J. | Automatic hopper transfer | X |  |  |
| K. | Maximum 120 VAC | X |  |  |
| L. | Maximum overall dimensions: 60'h x 35"w x 25'd | X |  |  |
| M. | Minimum of two (2) bill acceptors installed in unit, 24V MDB | X |  |  |
|  | -High-capacity magazine | X |  |  |
| N. | UL approved |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

BILL CHANGER (2 HOPPER)

Make & Model Number: \_\_\_\_\_\_\_\_MC200 CHANGER \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 2-hopper bill changer with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Front loading machine | X |  |  |
| B. | Maximum security design | X |  |  |
| C. | Minimum 14-gauge steel construction | X |  |  |
| D. | "T" handle type lock receptacles | X |  |  |
| E. | Minimum 2 hoppers accommodating: $1 coins, quarters, dimes, and nickels | X |  |  |
| F. | Accepts $1, $5, $10, and $20 bills | X |  |  |
| G. | Accepts Susan B. Anthony and $1 gold coins |  |  | X |
| H. | Hand-held data terminal for programming with braille |  |  | X |
| I. | Battery back-up |  |  | X |
| J. | Automatic hopper transfer | X |  |  |
| K. | Maximum 120 VAC | X |  |  |
| L. | Maximum overall dimensions: 60'h x 35"w x 25'd | X |  |  |
| M. | Minimum of one (1) bill acceptor installed in unit, 24V MDB | X |  |  |
|  | -High-capacity magazine | X |  |  |
| N. | UL approved | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

BILL CHANGER (1 HOPPER)

Make & Model Number: \_\_\_\_\_\_\_MC100 CHANGER \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 1-hopper bill changer with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Front loading machine | X |  |  |
| B. | Maximum security design | X |  |  |
| C. | Minimum 14-gauge steel construction | X |  |  |
| D. | "T" handle type lock receptacles | X |  |  |
| E. | Minimum 1 hopper accommodating: $1 coins, quarters, dimes, and nickels | X |  |  |
| F. | Accepts $1, $5, $10, and $20 bills | X |  |  |
| G. | Accepts Susan B. Anthony and $1 gold coins |  |  | X |
| H. | Hand-held data terminal for programming with braille |  |  | X |
| I. | Battery back-up |  |  | X |
| J. | Automatic hopper transfer | X |  |  |
| K. | Maximum 120 VAC | X |  |  |
| L. | Maximum overall dimensions: 60'h x 35"w x 25'd | X |  |  |
| M. | Minimum of one (1) bill acceptor installed in unit, 24V MDB | X |  |  |
|  | -High-capacity magazine | X |  |  |
| N. | UL approved | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

BILL ACCEPTOR, 24V MDB

Make & Model Number: \_\_\_\_\_\_CONLUX CV322-U5M\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured 24V MDB bill acceptor with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Accepts $1, $2, $5, $10, and $20 U.S. bills | X |  |  |
| B. | Accepts bills lengthwise, four ways (face up or down, either direction) | X |  |  |
| C. | 95% or greater acceptance rate for U.S. bills | X |  |  |
| D. | Options can be customized on location | X |  |  |
| E. | Re-programmable flash memory allows for software updating | X |  |  |
| F. | Bill capacity of 300 with optional 200, 500, and 700 stackers available | X |  |  |
| G. | UL approved | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

COIN MECHANISM

Make & Model Number: \_\_\_\_\_\_\_\_\_CONLUX MCM5-4\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured coin mechanism with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Accepts U.S. nickels, dimes, quarters, and dollar coins | X |  |  |
| B. | Pay out U.S. nickels, dimes, quarters, and dollar coins | X |  |  |
| C. | Token acceptance capability | X |  |  |
| D. | Maximum coin tube capacity: 74 quarters, 99 dimes, 67 nickels | X |  |  |
| E. | Self-test system diagnostics | X |  |  |
| F. | Multi-drop bus capabilities | X |  |  |
| G. | Control board protected from fluids | X |  |  |
| H. | 24V MDB | X |  |  |
| I. | UL approved | X |  |  |
|  |  |  |  |  |

MAGLINER (LARGE)

Make & Model Number: \_\_\_\_\_\_\_\_\_\_\_\_0-190-6020\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured Magliner, Gemini Sr. Convertible Hand truck, 10 in. Pneumatic wheels or acceptable equivalent with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Overall width, 21" | X |  |  |
| B. | Frame width, 12" | X |  |  |
| C. | Deck width, 12" | X |  |  |
| D. | Overall length, 4 wheel, 55-3/4" | X |  |  |
| E. | Height (as hand truck), 61" | X |  |  |
| F. | Height (as platform truck), 45-1/8" | X |  |  |
| G. | Platform bed length, 51" | X |  |  |
| H. | Platform height from floor, 10-1/2" | X |  |  |
| I. | \*Standard wheel, 10" | X |  |  |
| J. | \*Casters (standard swivel), 5" x 1-1/4" with wheel lock | X |  |  |
| K. | Nose, 18" x 7-1/2" | X |  |  |
| L. | Shipping weight, 45lbs | X |  |  |
| M. | Platform height from floor, 10-1/2" | X |  |  |
| N. | Nose, 18" x 7-1/2" | X |  |  |
| O. | Shipping weight, 45lbs | X |  |  |
| P. | Handle, horizontal loop (301000) | X |  |  |
| Q. | Die cast aluminum 18W x 7-1/2"D | X |  |  |
| R. | 10", 4ply pneumatic (121060) | X |  |  |
| S. | Minimum capacity (as hand truck), 500lbs | X |  |  |
| T. | Minimum capacity (as platform truck), 1000lbs | X |  |  |
| U. | Fully assembled |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

MAGLINER (SMALL)

Make & Model Number: \_\_\_\_\_\_\_\_\_\_0-190-6013\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured Magliner, Gemini Sr. Convertible Hand truck, 10 in. Pneumatic wheels or acceptable equivalent with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Overall width, 21" | X |  |  |
| B. | Frame width, 12" | X |  |  |
| C. | Deck width, 12" | X |  |  |
| D. | Overall length, 4 wheel, 47-1/2" | X |  |  |
| E. | Height (as hand truck), 51" | X |  |  |
| F. | Height (as platform truck), 40” | X |  |  |
| G. | Platform bed length, 38" | X |  |  |
| H. | Capacity (as hand truck), 500lbs | X |  |  |
| I. | Capacity (as platform truck), 1000lbs | X |  |  |
| J. | Platform height from floor, 10-1/2" | X |  |  |
| K. | \*Standard wheel, 10" | X |  |  |
| L. | \*Casters (standard swivel), 5" x 1-1/4" with wheel lock | X |  |  |
| M. | Nose, 18" x 7-1/2" | X |  |  |
| N. | Shipping weight, 44lbs | X |  |  |
| O. | Handle, horizontal loop (301000) | X |  |  |
| P. | Die cast aluminum 18W x 7-1/2"D | X |  |  |
| Q. | 10", 4ply pneumatic (121060) | X |  |  |
| R. | Fully assembled | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

LOCKING CASTER SETS

Make & Model Number: \_\_\_\_\_\_\_6650-25-XDP-TSB\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The following specifications are to be the minimum requirements as set forth by the Using Agency. Specifications used are intended to be open and non-restrictive. Any brand name reference is intended to establish criteria and quality guidelines for competitive bidding. Only those who can supply, install, and service this equipment should submit bids.

Newly manufactured locking caster sets with the following specifications:

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A. | Set of four (4) swivel casters with brakes | X |  |  |
| B. | 3" x 1-3/4" heavy duty polyolefin wheel with roller bearings | X |  |  |
| C. | 2800lb capacity per set | X |  |  |
| D. | 4-1/4" mounting weight height | X |  |  |
| E. | Heavy duty welded construction | X |  |  |
| F. | 1/2" -13 mounting stem | X |  |  |
| G. | Zinc plated | X |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**GENERAL SPECIFICATIONS APPLICABLE TO ALL EQUIPMENT**

YES NO

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. | Parts and service manuals shall be provided with each machine at time of delivery. | X |  |  |
|  |  | X |  |  |
| 2. | On-site training on each machine including the operation and cleaning procedures at time of delivery. | X |  |  |
|  |  | X |  |  |
| 3. | Equipment shall be uncrated, pre-tested, and set up according to manufacturer’s recommendation before delivery. Any equipment damaged in shipping or not working at delivery shall be replaced within 24 hours. | X |  |  |
|  |  | X |  |  |
| 4. | Equipment shall be delivered within a maximum of 30 days after receipt of purchase order. | X |  |  |
|  |  | X |  |  |
| 5. | Product brochure(s) and manufacturer’s specification sheets (cut sheets) for model offered shall be provided at time of bid. | X |  |  |
|  |  | X |  |  |
| 6. | Minimum manufacturer’s warranty against defects: 1-year parts, 90 days labor, with additional 1 year parts warranty and available from vendor in writing. Compressor warranties: minimum of 3 years. |  |  |  |
|  |  | X |  |  |
| 7. | Vendor shall respond on site within a maximum of 48 hours within warranty period to service requests (48 hours after warranty period). | X |  |  |
|  |  | X |  |  |
| 8. | All units shall be delivered and installed at no additional charge and leveled to operational status, including electrical and/or water hook-ups, to any blind vending site throughout all 92 counties of the State of Indiana. Specific delivery locations will be given with each Quantity Purchase Award Release (QPAR). | X |  |  |
|  |  | X |  |  |
| 9. | Used equipment shall be picked up as new equipment is delivered. Used equipment shall be taken to the state warehouse located at 6400 E. 30th St., Indianapolis, Indiana 46219, or state surplus, 601 W McCarthy St, Indianapolis, Indiana 46225, between the hours of 7:00am-4:30pm, Monday through Friday. Any charges for this service should be noted on bid. | X |  |  |
|  |  | X |  |  |
| 10. | Keys and locks shall be supplied with equipment at time of delivery. | X |  |  |
|  |  | X |  |  |
| 11. | New equipment shall be bolted in a bank with other equipment as needed. | X |  |  |
|  |  | X |  |  |
| 12. | Original manufacturers nameplate and serial number shall be stamped on each machine at time of delivery, or it will not be accepted. | X |  |  |
|  |  | X |  |  |
| 13. | Each bidder should submit with their bid a manufacturer's statement of dealer authorization certifying that his/her firm is an authorized distributor for the products being bid and that the appropriate machines meet the requirements of the 1990 Clean Air Act. | X |  |  |
|  |  | X |  |  |
| 14. | Service shall be performed by manufacturer's authorized service technicians. | X |  |  |
|  |  | X |  |  |
| 15. | Any braille on keypads that is requested on any machine must be maintained by the vendor for the life of the machine. |  |  | X |