0.01	50	100.00	PASS	Maximum thermal cracking at reliability
549.730866926863	95	100.00	PASS	Maximum total transverse cracking at reliability
0.471027803219823	95	81.65	FAIL	Maximum AC Rutting at reliability
1.12937792851226	95	11.69	FAIL	Maximum total Rutting at reliability
1143.04653214632	95	99.80	-	Maximum Top Down Cracking at reliability
2.05E-12	50	100.00	PASS	Maximum Bottom up Cracking at reliability
37.0983	95	0.00	FAIL	Maximum total fatigue cracking at reliability
179.741441808631	95	85.60	FAIL	Maximum Terminal IRI at reliability
