40	Analysis Type
70.000	InitialIRI
95	IRI Reliability
50	Bottomup Cracking Reliability
95	Top Down Cracking Reliability
50	Thermal Reliability
50	CTB Reliability
95	AC Rutting Reliability
95	Total Rutting Reliability
90	Reflective cracking reliability
0.24 * Pow(RUT,0.8026) + 0.001	AlphaRutAC
70.98 * Pow(TRANSVERSE,0.2994) + 30.12	ReflectiveCrackingACTransverseStandardDeviation
0.1477 * Pow(BASERUT,0.6711) + 0.001	BaseSTD
0.1235 * Pow(SUBRUT,0.5012) + 0.001	SubgradeSTD
200 + 2300/(1+exp(1.072-2.1654*LOG10(TOP+0.0001)))	AlphaTop
1.1097 * Pow(FATIGUE,0.6804) + 1.23	ReflectiveCrackingACFatigueStandardDeviation
CTB*11	AlphaCTB
40	IRI_GBC1
0.4	IRI_GBC2
0.008	IRI_GBC3
0.015	IRI_GBC4
40.8	IRI_ATBC1
0.575	IRI_ATBC2
0.0014	IRI_ATBC3
0.00825	IRI_ATBC4
16	Plasticity Index
93.5	Passing #4
63.2	Passing #200
10	fatigueBottom
2000.000	fatigueTop
500.000	thermalFracture
25	CTB
0.400	ruttingAC
0.750	ruttingTotal
160.000	iRI
25.000	reflectiveCrack
95.000	reliabilityReflectiveCrack
2500.000	transverseReflectiveCrack
95.000	reliablityTransverseReflectiveCrack
100.000	AmountExistingTransverseCracking
120	ReflectiveCrackingSemiTransverseM
