

PLAT NO. 1 CHECKLIST

	No.
	Requirement Description
	Included

	1.
	Section corner tie-in included if project did not have a Location Control Route Survey Plat.
	[bookmark: Check1]|_|

	2.
	Section corners, section lines, and quarter-section lines identified.
	[bookmark: Check2]|_|

	3.
	For all properties impacted by the proposed construction, property owners identified and apparent property lines shown, but not labeled as such.
	[bookmark: Check3]|_|

	4.
	Name of stream, river, etc., identified, with flow direction.
	[bookmark: Check4]|_|

	5.
	Civil township; and section, township, and range; and county identified.
	[bookmark: Check5]|_|

	6.
	Stations shown in 100-ft increments.
	[bookmark: Check6]|_|

	7.
	All right-of-way lines shown and identified. Stations and offsets for right-of-way points should not be shown.
	[bookmark: Check7]|_|

	8.
	All temporary right-of-way shown and labeled, if applicable. The purpose for temporary right-of-way need not be specified.
	[bookmark: Check8]|_|

	9.
	Line designation of project centerline and all S-lines identified. Centerlines shown from which the new right-of-way is described.
	[bookmark: Check9]|_|

	10.
	Stations and locations of begin-project and end-project points identified.
	|_|

	11.
	All station equations shown and labeled.
	|_|

	12.
	Applicable subdivision names and lot numbers identified, if applicable.
	|_|

	13.
	North arrow shown.
	|_|

	14.
	Drawing scale indicated.
	|_|

	15.
	Existing roads shown and labeled.
	|_|

	16.
	Landlocked residues identified with crosshatching, if applicable.
	|_|

	17.
	Hexagon frame used around numbers for property owner legend and index, if applicable.
	|_|

	18.
	All mitigation sites delineated and labeled, if applicable.
	|_|
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