400-R-680 QC/QA SAMPLING AND TESTING ON 401 AND 410 PAY ITEMS

*(Adopted 06-21-18)*

 Each location shown in the table below that has a quantity less than 300 t per item number will be accepted by a type D certification in accordance with 402.09. Compaction of mixtures at locations shown in the table below that have an original contract pay item quantity less than 300 t per item number shall be in accordance with 402.15, except rollers shall not be operated in vibratory mode for mixtures in accordance with 410.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Pay Item Number |       |       |       |       |       |       |       |
| Pay Item Description |       |       |       |       |       |       |       |
| Des No. and Location |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |